(footprint "alignment_pin_1.5mm" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 62A3D9F7)
  (attr through_hole)
  (fp_text reference "REF**" (at -4.9 -0.035 unlocked) (layer "F.SilkS") hide
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 3c81aedc-1695-49db-9a83-a20936e7c5ff)
  )
  (fp_text value "alignment_pin_1.5mm" (at 0.365 4.035 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp b992e44a-204b-4254-98e0-e32c93f9d0b2)
  )
  (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp bf67bead-7707-485e-9d7d-4173d0bc7512)
  )
  (fp_circle (center 0 0) (end 0.75 0) (layer "B.Paste") (width 0) (fill solid) (tstamp d83d0af5-752a-420d-bbc7-b7ae13d3a568))
  (fp_circle (center 0 0) (end 0.75 0) (layer "F.Paste") (width 0) (fill solid) (tstamp 172527cb-120f-4525-acd5-b5b2524d9ff4))
  (pad "" np_thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1.5) (layers F&B.Cu *.Mask) (tstamp 4c66e059-dd09-42b2-9a4a-9d36af00adcf))
)
