(footprint "MAX17222ELT+T" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 61E64D0F)
  (attr smd)
  (fp_text reference "REF**" (at -2.025 -1.365 90 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 45245258-c97a-4586-bc43-2154c85c0ef6)
  )
  (fp_text value "MAX17222ELT+T" (at 5.315 1.485 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 1bb16fed-1537-47fa-90f6-8dc136da5d16)
  )
  (fp_text user "${REFERENCE}" (at 1.25 0.03 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp dd01ca49-c8a2-4580-af9a-2e9bce9769bc)
  )
  (fp_rect (start -1 -1) (end 1 1) (layer "F.SilkS") (width 0.12) (fill none) (tstamp a0d41751-5d18-4c9f-b863-fe47b2319611))
  (fp_circle (center -1.305 1.45) (end -1.052314 1.45) (layer "F.SilkS") (width 0.12) (fill solid) (tstamp b7e9cf10-b74e-4e80-a7f1-e33a29fe56de))
  (pad "1" smd rect (at -0.65 0.915 90) (size 0.8 0.35) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 8a1a639a-559c-483d-9c99-1b2fafbdacf1))
  (pad "2" smd rect (at 0 0.915 90) (size 0.8 0.35) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp a3eaa329-1c23-49fc-9fb5-976de81b788e))
  (pad "3" smd rect (at 0.65 0.915 90) (size 0.8 0.35) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp fab79269-47fb-42f7-a3ad-b9ec94b79b4b))
  (pad "4" smd rect (at 0.65 -0.915 90) (size 0.8 0.35) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp ccdce88e-24b7-4692-934b-22bb9b0763dc))
  (pad "5" smd rect (at 0 -0.915 90) (size 0.8 0.35) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp a9fdce30-e0b1-49dc-914c-0573fb33fbc7))
  (pad "6" smd rect (at -0.65 -0.915 90) (size 0.8 0.35) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 1c6c46b2-dd9e-430f-85e9-621815ceca94))
  (model "${KIPRJMOD}/3d/21-0164B_L622-1_MXM.step"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 -90))
  )
)
