(footprint "FP1005R1-R15-R" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 0)
  (attr smd)
  (fp_text reference "REF**" (at -3.01 -4.43 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 7e560f4d-9a5a-4df8-aeb5-6950834c9712)
  )
  (fp_text value "FP1005R1-R15-R" (at 7.11 4.39 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp e44652d2-5320-4f2d-af2b-816e53cd2df8)
  )
  (fp_text user "${REFERENCE}" (at -3.12 4.43 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 42f0e44d-d84a-4f88-8fbe-0a4d12b90453)
  )
  (fp_rect (start -5 -3.5) (end 5 3.5) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 772b6c77-5e80-45ba-b38d-0b8f2122d90a))
  (pad "1" smd rect (at -4.16 0) (size 2 3.1) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 1df999cf-fdfe-4eff-8f63-64030b8110d6))
  (pad "2" smd rect (at 4.16 0) (size 2 3.1) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp be043bc6-ba6a-4fa4-8d64-2f48156a80f9))
)
