(footprint "ST4ETB202" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 0)
  (attr smd)
  (fp_text reference "REF**" (at -3.3 0.4 90 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp ff357bb8-0628-4403-b4be-b1ea4ac70ed9)
  )
  (fp_text value "ST4ETB202" (at 7.22 -1.23 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp f81201e2-97d9-483e-80b1-08f10f408ef0)
  )
  (fp_text user "${REFERENCE}" (at 5.48 0.36 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp c433061f-a5c3-4ff3-91eb-eb314e2c4b88)
  )
  (fp_rect (start -2.25 -2.5) (end 2.25 2.5) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 06becf44-7f4a-4b5b-be2e-a9c1a70665df))
  (pad "1" smd rect (at 1.16 3 90) (size 2 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 21b4a24f-ea87-42b6-b7a9-0329259d5e47))
  (pad "2" smd rect (at 0 -3) (size 2 2) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 6c17ee7d-80f2-4ad5-aed8-c0fe33a350ea))
  (pad "3" smd rect (at -1.16 3 90) (size 2 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 0ceab0d0-a13e-4a79-b197-6e5cd6ebba02))
)
